AutoGen X Legacy to X_Pro Migration
Windows USB Driver Notes

This controller is expected to appear as a Silicon Labs CP210x USB-to-UART bridge on Windows.

If the migration tool does not find a COM port:
1. Unplug the controller.
2. Install the Silicon Labs CP210x VCP driver.
3. Reboot Windows if prompted.
4. Plug the controller back in with a USB data cable.
5. Open Device Manager and confirm a new COM port appears under:
   Ports (COM & LPT)

Expected names usually include one of:
- Silicon Labs CP210x USB to UART Bridge
- CP210x USB to UART Bridge

If no COM port appears after driver install:
- Try a different USB data cable.
- Try a different USB port.
- Avoid USB hubs.
- Then run the migration tool again.
