AutoGen X Legacy to X_Pro Migration Tool

This package is only for migrating a legacy AutoGen X controller to X_Pro over USB.

What it flashes:
- bootloader.bin @ 0x1000
- partitions.bin @ 0x8000
- boot_app0.bin @ 0xE000
- firmware.bin @ 0x10000

Windows users:
- If the controller does not appear as a COM port, install the Silicon Labs CP210x driver first.
- See WINDOWS_DRIVER_INSTALL.txt.

How to use:
1) Plug the controller into USB with a data cable.
2) Run the migration tool.
3) Wait for the success message.
4) Power-cycle the controller.

Do not use this package for normal legacy firmware updates.
